| **Available in** | **Plastic** | **Carbon** |
| --- | --- | --- |
| **Wheel diameter** | 24″ | |
| **Maximum permissible camber** | 3° | |
| **Load-bearing capacity of wheelchair** | 150 kg | |
| **Axle** | Quick-change axle 2 bearings for enhanced stability | |
| **Weight of segment** | 1030 g | 1290 g |
| **Design** | Spoke wheel, matt surface, black | High-gloss carbon disc, black |
| **Special feature** | The robust trivida wheel in reliable plastic quality offers an optimal price-performance ratio. | The high-strength trivida carbon wheel in the modern design impresses with its accurate handling and particularly long life. |
| **Guarantee** | 24 months | |
| **Certification** | CE | |
| **Scope of delivery** | Quick-change axle: ø 12 mm with 50 mm insertion depth Compatible assembly bush M16 with 50 mm insertion depth Bushes for 1/2″ axle system Stainless steel nut M16 | |